Version 7.02 (April 25, 2003)
--------------------------------------------------------------------------
This file contains information regarding the corrections, modifications 
and enhancements that have been made since the release of version 7.01.
--------------------------------------------------------------------------

Table of Contents:
1. New Features & Enhancements
2. Bugs and Fixes
3. Printer-Specific Fixes and Corrections
4. New Drivers

--------------------------------------------------------------------------


1. New Features & Enhancements:
-------------------------------

- LABELVIEW 7.02 Gold edition includes one license for the new Pocket 
  LABELVIEW application for Windows CE terminals and Pocket PCs. Pocket 
  LABELVIEW allows you to take labels created in LABELVIEW 7.02 Gold, 
  download them to your Win CE/Pocket PC device, and print them using a direct 
  or network/wireless connection.

- In addition to its NATIVE support for hundreds of LABELVIEW printer drivers, 
  LABELVIEW 7.02 also includes the entire TEKLYNX family of drivers. 

  Depending on the printer you are using, there may be several driver 
  choices available in the software. Some printers include both a native 
  LABELVIEW driver and a TEKLYNX driver for the same printer model, designated 
  in the program with a "(V)" for native LABELVIEW drivers or a "(X)" for the 
  extended TEKLYNX drivers. You may want to try all of the drivers available for 
  your particular printer model and determine which one works best for your 
  label printing needs.

- Several improvements have been made to Print Station:
  * When sending print jobs to Print Station, you can now queue (suspend) 
  the jobs and release them later (vs. having to print the jobs immediately).

  * When printing via Print Station, the "WHEN" value (ASAP, Timed, or Suspend)
  will be remembered the next time the Print window is opened.



2. Bugs and Fixes:
------------------
========
GENERAL
========

- Fixed issue with Logging feature not logging field values, only the quantity. 
  (CTHS-5JJRJD)

- The functions mod10() and addmod10() now work correctly. (SRUO-5HEF49)

- When printing a label to a picture file, the human readable text will now 
  print correctly. (THAN-5D3JXA)

- Fixed issue where the program would crash on exit if an OLE object is 
  edited by double-clicking on it. (CHUR-5ESKJW)

- Removed Add Shape capability in both Pro and Gold Run-Time versions. 
  (MSTA-5GQT2Q)

- A user with no rights could add shapes. This capability has been removed.
  (MSTA-5GQSUB)

- Fixed issue where a label created under LABELVIEW 5.41, when opened with 7.0, 
  would shift the text positions in some cases.(PSCZ-5EPMAU)

- Fixed issue where any query string (either valid or invalid) would cause 
  LABELVIEW to crash when the Test button is pressed. If Test is not pressed but 
  saved instead, LABELVIEW would crash when viewing the print grid. 
  (KRON-5DTUQ5)

- Fixed issue where program would crash in Windows 98 if no printers were 
  installed and no HASP key was installed. (SGRC-5E6Q6N)

- Fixed issue with Autofind (and Browse) button when trying to find the license 
  server. (SGRC-5ELJMP)

- Fixed error appearing in Windows 2000 and XP when trying to install or connect 
  to a shared printer via the Add Port button. (SGRC-5ELMDA)

- When opening a label from the internet, the user can now select a default 
  directory on the ftp site. (KRON-5DTUV3)

- Removed improper compliance samples

==========
BAR CODES
==========

- Fixed issue with some 2D bar codes not rotating correctly. (RKOI-5JQLNQ)

- In the Aztec Mesa Composite Text Window, the word-wrap is now being utilized 
  so the user can view the entire string. (CHUR-5EQMLF)

- Code 128C(F1 Mod 10) now creates the correct check digit if the value 
  0000000000000000116 is used. (MSTA-5EWM9M)


==========
PRINTING
==========

- Fixed WYSIWYG issue where label was shifting to the right when printing to 105 
  SL printers. (JGAO-5HULBP, MMUR-5GSSFC)

- Fixed issue where thermal LABELVIEW drivers were activating the Windows 
  spooler when selecting direct printing and print station. The default has 
  now been set to USE WINDOWS PRINT MANGER when running on NT. (BLUI-5HRMHV)

- Fixed issue when using the Customize Bar Code Human Readable with a Code 39
  bar code. If the label is stored in the printer memory for later recall, upon 
  printing this stored label the human readable shifts and prints a " before and 
  after the human readable text. (BLUI-5ERJNY)

- Fixed issue occurring when label is set to print 4 across and cut after 12 
  labels (after the 3rd row). If one record (with a quantity of 12) is selected 
  from the database, it would cut in the proper location. If more than one 
  record is selected it would cut after every row. (MSTA-5CYL3A)

- Program will now send the correct commands when setting the sensor type to 
  black mark in the label setup. (THAN-5JVK53)


=======
FONTS
=======

- Labels using SanSerif font will no longer change font to Arial. (5HEJTB)

- TrueType fonts and graphics now print correctly. (PSCZ-586KNE)

- Paragraph text settings for alignment and left justification are now printing 
  correctly when using TrueType fonts. (THAN-5JWM4G)


====================
WHEN PRINTED FIELDS
====================

- Fixed issue occurring with When Printed fields when changing the string
  length to something other than the default (10). If you then change the 
  font, the string length would go back to the default. (MSTA-5GWKCZ)

- Fixed issue occurring when the number of When Printed fields is greater 
  than 8 and they are REQUIRED. The user was able to leave fields blank for 
  those fields not showing on the Quick Printing screen. (BLUI-5GQL46)


=================
DATABASE AND SQL
=================

- Improved SQL statement support. (BLUI-5HRNAY)

- Fixed issue occurring when records in database columns are not complete. The 
  data was being randomly printed/missed on the label and empty fields in a 
  record were causing the wrong value to be printed. (JKAO-5JJLXS)

- Program no longer crashes when custom SQL string length exceeds approximately 
  120 characters. (KRON-5DTKTW)



=======================================
DATAWATCH, COMMWATCH AND COMMAND FILES
=======================================

- Fixed issue with DataWatch where it would not print new records when the 
  Quantity data source was set to anything other than When Printed. The 
  monitoring screen was recognizing a change and logging records as being 
  printed, but no job was being spooled to the printer. (CTHS-5J9J8C)

- Fixed issue with DataWatch and command files occurring if the time interval 
  for command files was set to zero. (KRON-5DVTYN)

- When using DataWatch with Oracle, program will now print new records. 
  (TDIN-5GJQSJ, RMCE-5FMHYB)

- CommWatch will no longer generate an error when using carrier detect line 
  signal with Win2000. (MCHN-5ERPGT)

- Fixed issue occurring when using command files where every time the monitor 
  prints a label, the program would change the name of the directory it was 
  monitoring. (RMCE-5J9KG5)


=========
PRINTPAD
=========

- Fixed issue occurring when trying to download over 999 labels from the 
  PRINTPAD CE to a Sato printer. When using a When Printed field the quantity 
  was being restricted to 999 labels from the PRINTPAD CE. (THAN-5HEJQT)

- Fixed issue occurring when printing labels from the PRINTPAD with a Quantity 
  data source set to Database. The PRINTPAD will no longer prompt for the 
  quantity (quantity should be coming from the database). (THAN-5HENY4)

- Fixed issue occurring when trying to print labels from the PRINTPAD with a 
  Quantity data source set to Constant. After selecting the label to print, the 
  PRINTPAD would display Field Count=0, and then go directly back to the screen 
  for selecting a label without printing the label. (THAN-5HENVZ)



3. Printer-Specific Fixes and Corrections:
------------------------------------------

QuickLabel Systems models
- Created a new manufacturer group and moved the printers there

Avery Dennison 6404 bit series 924, 925, 926, dpm 4, dpm 5, and dpm 6
- Graphics no longer print as mirrored images when the "Print binary graphics as 
  graphics" option is selected. (BLUI-5HNPKM)

C.ITOH S4
- Print Preview no longer cuts off the last part of the image in some bar codes.
  (BLUI-5G2KRQ)

Datamax E4304 
- Made change in heat setting to allow 0-30. (PSCZ-5HTB6S)

Datamax I4308
- Cutter now cuts correctly when the cutter is set to cut after each label.
  (RMCE-5D9JRB)

Printronix T520X, T530X
- Advanced gap and advanced notch label sensing types have been added.
  (RMCE-5F8FQ6)

Printronix T5306
- Shapes will now print on the Printronix T5306 printer. (KRON-5EKSCR)

Tec CB 416 4-Color
- Added a check box "Use printer Fine Adjust X/Y Setting" on the
  Label Setup / Color tab for the color printer. User can now check the 
  check box to turn off the setting from LABELVIEW and use the printer 
  settings. (RKO1-51BHH7)

Zebra 105SE 300 dpi
- Black mark sensor labels will now print properly. (THAN-5JEJXX)

Zebra 105SL
- Printed objects are no longer shifted over to the right. (RKOI-5GJRT5)

Zebra DA402
- Added the ability to adjust the heat. (MSTA-5C4SQG)



4. New Drivers:
---------------
Version 7.02 includes new printer drivers for models from the following 
manufacturers:

ADC
Allen
Anritsu
Argox
Astro-Med
AT&T
Avery
Axiohm
Bancolini
Brady
C.Itoh
CAB
Carl Valentin
Citizen
Codewriter
Cognitive
Comstar
Comtec
Datamax
DH/Cognitive
Eltron
Facit
Fox IV
General Code
IBM
IER
Imaje
Impuls
Intermec
Investix
Ishida
ITW
K-Roll
Legi
Leptons
Logopak
Markem
Markpoint
Meto
Microcom
Microplex
Monarch
MPH
Novexx
Open Date
Paxar
Pressiza
Printronix
RHS
Ricoh
RJS
Sato
TEC
Thermo-Tex
TSC
TTF
UBI
Vitadresse
Wilux Print
Zalton
Zebra



=========================================================================
=========================================================================


Version 7.01 (December 2, 2002)
--------------------------------------------------------------------------
This file contains information regarding the corrections, modifications 
and enhancements that have been made since the release of version 7.0.
--------------------------------------------------------------------------

Table of Contents:
1. New Features & Enhancements
2. New Drivers
3. Bugs and Fixes

--------------------------------------------------------------------------


1. New Features & Enhancements:
-------------------------------

Version 7.01 includes support for the PRINTPAD CE bar code printing terminal.


2. New Drivers:
---------------

TSC TTP-2412M 
TSC TTP-245 
TSC TTP-246M 
TSC TTP-248M 
TSC TTP-344M 
TSC TDP-643Plus


3. Bugs and Fixes:
------------------
 
- Fixed issue where the Label Designer would crash when running on Win95 on 
  some PCs. Windows 95 users using the PRINTPAD 2000/4000 must install the 
  WS2_32.DLL file, which can be downloaded from http://support.microsoft.com.

- Label Select will no longer lose its path when trying to load a label.

- Label Select would not load the label if a specified printer alias was not
  found. In version 7.01 a warning will pop up, allowing the user to continue.

- When Printed fields using Center Justification on the PRINTPAD 500 will now 
  print in the correct position on Eltron printers.

- Printer resident fonts with Center Justification will now print correctly on
  a SATO CL408e.

- Fixed issue where selecting to print a run separator on a Zebra printer 
  would cause a blank label to be printed.
  
- When activating all Diagnostics settings, the "Print printer commands to"
  setting lists only Windows drivers for selection. When printing any label this
  would cause LABELVIEW to crash. This has been fixed.


=========================================================================
=========================================================================


Version 7.0 (September 20, 2002)
--------------------------------------------------------------------------
This file contains information regarding the corrections, modifications 
and enhancements that have been made since the release of version 6.09.
--------------------------------------------------------------------------

Table of Contents:
1. New Features & Enhancements
2. New Drivers
3. Bugs and Fixes
4. Printer-Specific Fixes and Corrections

--------------------------------------------------------------------------


1. New Features & Enhancements:
-------------------------------

- New "Shape" feature allows users to add a variety of shape types (Arrows,
  Packaging, Tools, etc.) to their labels. Users can also add their own custom
  company- or industry-specific graphics as shapes by creating a Windows
  Metafile and saving it in a sub folder within the program's Shapes folder.

- HIB Barcode (HealthCare Barcode) added as a checkbox on the Configuration
  dialog's Display tab. If the "Use HIB Barcode" option is checked, a button
  will appear at print time. Users can click this button to access the HIB 
  Barcode input dialog box.

- New 2D bar codes added: Aztec, Aztec Mesa, Code 49, Data Matrix, MicroPDF, and 
QR Code.

- The program now supports File DSN, allowing you to store the DSN parameters
  in a text file so you can easily distribute the file from one PC to another 
PC.

- SQL button added to the Text and Barcode dialogs allows you to add a 
customized 
  SQL statement for an ODBC data source.

- The "Multiple Raw Data" command file mode is now supported. The Multiple Raw 
Data
  command file type allows you to store variable data for command files outside 
the
  command file itself, instead of internally.

- Support for the new PRINTPAD CE has been added to this version.



2. New Drivers:
---------------

- Sato RVe 

- Zebra 105SL/203 

- Zebra 105SL/300



3. Bugs and Fixes:
------------------

- Fixed problem with editing files and adding records to a file in the internal
  Database Editor.

- Fixed problem When using a SUBSTR linked expression that has another nested
  expression in it and it is linked to a CommWatch field. An  error was being
  generated at print time : "1112=Syntax Error in SUBSTR :  parameter number 3
  should be numeric."

- Fixed Problem of HEX link expression when converting a decimal value.

- UPC-A bar code created as a When Printed field and printed to a picture no
  longer shows all zeros in the human readable.



4. Printer-Specific Fixes and Corrections:
------------------------------------------

- BellMark: UCC-EAN 128 MULTI bar code support has been added.

- Datamax: Printer real time and date stamps support has been added to all 
  printers that support this feature.

- Eltron 3742: Fixed so no longer switches a 128B bar code to a 128 Auto
  Switching after saving the label and reopening the label. 

- Printronix T5306: Fixed problem occurring when trying to print graphics 
greater
  than 6x6 inches.

- Sato: Printer real time and date stamps support has been added to all printers
  that support this feature.
  
- TEC 472: Fixed problem occurring if first character of a line is printed 
  incompletely when using an upside-down print orientation.

- Zebra 105: When "printing to picture" the bar code human readable no longer
  displays as X's. 
  
